Configuration............. |

Hardware connections:

- Connectors:
Better do not connect or disconnect cables while module is running
First disconnect module from power supply and then do configuration works afterwards.
- Electrostatic protection:
Protect the module from overvoltage by electrostatic charge.

Configuration via Webbrowser:

Select the menu entry on the left menu page to configure the different interfaces (CAN, COM1, etc.).
For every interface there is a own sub menu.

The configuration generally takes place in three steps:

1. Configure the selected interface (CAN, COM1, etc..) over the available GUI of elements like text fields, radio button or select boxes. To restore the original settings press "Reset" button.
2. Press "Submit" button to submit the settings to CAN2Web module.
3. A web page with the changed settings appears.

Storing of settings:
To store the settings select menu "Option" in the left menu. Use the "Store" Button to store settings on file system. All settings will be loaded automatically after a Reset.

© synertronixx 2007